# ID 1001150

Number of configured expression labels exceeds the upper limit.
Description | The number of expression labels is defined in the channel parameter P-CHAN-00516. The configured value is greater than permitted.
Response | Class | 1 | Output of warning: Apply the permitted maximum value.
Solution | Class | 1 | Check and modify P-CHAN-00516
Parameter | %1: | Current value [-]
Configured value for P-CHAN-00516
%2: | Corrected value [-]
Corrected value for P-CHAN-00516
Error type | -