# ID 46033

Invalid pointer to a control unit of an axis group.
Description | The function block is to send a job for an axis group. To do this, it requires a pointer for access to a control unit of an axis group. However, the pointer is invalid.
Response | Class | - | Function block sets his output "Error" to TRUE and displays at output "ErrorID" the error number. Access is prevented to the control unit, and the function block does not send an axis group job to the motion controller.
Solution | Class | - | Please contact your motion control supplier.
Error type | -