# Version identifier of visualisation data (P-STUP-00039)

P-STUP-00039 | Version identifier of visualisation data
Description | The parameter sets the type of data structure which the contour visualisation ([FCT-C17]) supplies. Depending on the setting selected, more or less visualisation data is generated. An overview of existing data structures is contained in [FCT-C17].
Parameter | contour_visu_ifc_version
Data type | UNS32
Data range | contour_visu_ifc_version | Data structure
0 | SOLLKONT_VISU_DATA_V0 (default)
1 | SOLLKONT_VISU_DATA_V1
2 | SOLLKONT_VISU_DATA_V2
3 | SOLLKONT_VISU_DATA_V3
4 | SOLLKONT_VISU_DATA_V4
5 | SOLLKONT_VISU_DATA_V5
6 | SOLLKONT_VISU_DATA_V6
7 | SOLLKONT_VISU_DATA_V7
8 | SOLLKONT_VISU_DATA_V8
9 | SOLLKONT_VISU_DATA_V9
10 | SOLLKONT_VISU_DATA_V10
11 | SOLLKONT_VISU_DATA_V11
Dimension | ----
Default value | 0
Remarks |