# ID 50608

The order of the velocity filter is odd numbered.
Description | The order of the velocity actual value filter (P-AXIS-00623) is assigned an odd value; this will be corrected.
Response | Class | 1 | Warning and correction of parameter.
Solution | Class | 1 | Parameterise P-AXIS-00623 with an even number.
Parameter | %1: | Logical axis number [-]
%2: | Current value [-]
%3: | Corrected value [-]
Error type | 2, Error message by data transfer from parameter list into control device.