# ID 270061

Given destination state in transition not allowed.
Description | A job to change the state or an operation mode to change the operation mode itself requires specification of the required target state. The job that leads to this message contains a target state which is not permissible for the required operation mode.

The following target states are permissible for the automatic (2), manual block input (3), manual (4) and homing (5) operation modes

Operation mode state | Value
Deselected | 1
Selected | 2
Ready | 3
Active | 4
Hold | 5
Resetting | 15
The permissible target states for the Standby (1) operation mode are:
Operation mode state | Given destination state in transition not allowed.
Deselected | 1
Selected | 2
Ready | 3
Response | Class | 3 | The transition will not be executed
Solution | Class | 1 | Correct the destination state and start new request
Parameter | %1: |
Selected destination state
%2: |
Current operation mode
Error type | -