# ID 70342

Error in axis-specific transformation.
Description | An axis-specific command value transformation is activated P-AXIS-00380. The error can only occur because missing or incomplete parameter settings occurred in an axis-specific command value transformation. For more information on this function, see [AXIS// Section: Command value transformation].
Response | Class | 5 | Error message output, abort program.
Solution | Class | 6 | Check the parameter settings for the selected axis-specific transformation.
Parameter | %1: |
Logical axis number P-AXIS-00016 of axis affected.
%2: |
Info variable
%3: |
Current selected transformation ID.
Error type | -