# ID 20814

Measuring offset was not included into the programmed axis.
Description | It is not possible to calculate the measuring offset with command G102 in the programmed axis because no measuring offset has been calculated. [PROG// Section: Calculating measuring offsets (G101/G102
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check the programming of offsets (G101).
Parameter | %1: | Logical axis number [-]
Logical axis number (P-AXIS-00016)
Error type | 1, Error message from NC program.