# ID 50354

SERCOS-Parameter: Unknown SERCOS ID.
Description | Read or write command for SERCOS parameter in CNC program via #IDENT WR[], #IDENT RD[] failed because of unknown or invalid SERCOS-ID. For more information on this function see [PROG// Section: Writing and reading SERCOS parameters and commands].
Response | Class | 4 | Movement stop.
Solution | Class | 6 | Check SERCOS-ID in CNC program.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Identification number [-]
Programmed SERCOS ident number.
%3: | Current value [-]
SERCOS return value 1.
%4: | Current value [-]
SERCOS return value 2.
Error type | 1, Error message from NC program.