# ID 21994

Path from startup-list will be ignored.
Description | The program paths of NC channels can either be configured in the channel lists (P-CHAN-00401 to P-CHAN-00404) or in the start-up list (P-STUP-00018 to P-STUP-00021). Then the program paths in the channel lists are given priority. The transfer of program paths from the start-up list is discarded, The controller start-up is continued.
Response | Class | 1 | Warning, no reaction.
Solution | Class | 6 | Delete the configuration of the program paths for the channel from one of the two lists before the next start-up.
Parameter | %1: | Error value [-]
Path from start-up list
%2: | Error value [-]
Logical path number
%3 | Error value [-]
Path priority
%4 | Error value [-]
Path type
Error type |