# ID 44076

FB error: MCV_ConveyorControl; Value at input "ControlMode" is invalid.
Description | There is an invalid value assigned to input "ControlMode" of function block MCV_ConveyorControl. Allowed values at input "ControlMode" are:
Global constant | Value
HLI_CONVEYOR_SPEED_CONST | 0
HLI_CONVEYOR_ACCELERATION | 1
HLI_CONVEYOR_DECELERATION | 2
HLI_CONVEYOR_SPEED_ZERO | 3
HLI_CONVEYOR_MACH_WITH_SPEED_ZERO | 4
Response | Class | - | The invalid value is not sent via the appropriate control unit to the motion controller.
Solution | Class | - | Correct the assigned value. The corrected value is sent immediately to the motion controller if input "Enable" is TRUE.
Error type | -