# ID 150090

Invalid resolution of handwheel parameterised.
Description | In the manual mode parameter data record, the value 0 was parameterised for at least one of the parameters P-MANU-00005 or P-MANU-00006. Together these parameters define a handwheel resolution.
Response | Class | 3 | Manual mode parameters are not transferred to the CNC and start-up of CNC system is aborted.
Solution | Class | 6 | Correct the values of P-MANU-00005 or P-MANU-00006.
Parameter | %1: | Current value [-]
Value of parameter P-MANU-00005 or P-MANU-00006.
%2: | Logical identifier of control element [-]
Logical control identifier of the handwheel with the incorrect parameter.
Error type | 2, Error message on data transfer of parameter lists to controller.