# ID 21898

Movement block without angle programmed.
Description | A contour path consisting of 2 blocks is to be programmed. The second motion block was programmed without an angle. Programming this angle is necessary. Example with error: N240 G17 G01 X10 Y5 N250 #RND=3 N260 #ANG=30 #RND=4
N270 G01 X30 Y25

Corrected example:

N240 G17 G01 X10 Y5
N250 #RND=3

N260 #ANG=30 #RND=4
N270 #ANG=80 G01 X30 Y25

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the contour path in NC program. Add the necessary angle.
Error type | 1, Error message from NC program.