# ID 20154

Value following 'M' is out of data format.
Description | The programmed number of the M function exceeds the permissible data range. Example: Wrong: N10 G00 X0 Y0 Z0 N20 M150000

N1000 M30

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify NC program. Programmed number of M function must be within the permissible value range. Make sure that the M function is configured in the channel parameters P-CHAN-00041.
Parameter | %1: | Error value [-]
%2: | Limit value [-]
%3: | Limit value [-]
Error type | 1, Error message from NC program.