# Behaviour with messages to HMI (P-CHAN-00519)

P-CHAN-00519 | Behaviour with messages to HMI
Description | This message defines the behaviour with messages sent via the NC command #MSG to the HMI,
Parameter | configuration.decoder.msg_to_hmi
Data type | STRING
Data range | STANDARD : Messages to receiver HMI are written. DISABLED : Messages to receiver HMI are discarded. WARNING : Messages to receiver HMI are discarded and a warning (ID 22194) is output. ERROR : Messages to receiver HMI are discarded and an error (ID 22195) is output.
Dimension | ---
Default value | STANDARD
Remarks | Parameter available as of CNC Build V2.11.2059, V2.11.2830, V3.1.3079.43 or V3.1.3107.33.