# Velocity scaling factor (P-AXIS-00379)

P-AXIS-00379 | Velocity scaling factor (PROFIDRIVE)
Description | Thiss parameter supplies the velocity scaling factor set in the drive to the CNC. This value can be read with a drive set-up tool from the drive and has to be entered in this parameter. For SIMODRIVE 611 drives it is the parameter P880, for SINAMICS drives it is parameter P2000.
Parameter | antr.profibus.drive_velocity_base_value
Data type | UNS32
Data range | 1 … MAX(UNS32)
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | 16384
Drive types | Profidrive
Remarks |