# Path to the enveloping bodies (P-SECO-00002)

P-SECO-00002 | Path to the enveloping bodies
Description | This element specifies the path to the enveloping bodies which are monitored for collision. It can be specified as both absolute and relative. The length of the path is limited to 103 characters.
Parameter | path_to_geometry
Data type | STRING
Data range | Maximum of 103 characters
Dimension | ----
Default value | *
Remarks | * Note: The default value of variables is a blank string.