# ID 21400

Global feed weighting is programmed negative.
Description | The global feed weighting value programmed with G129 for rapid velocity is negative. Example: Wrong: N10 G00 X0 Y0 Z0 N20 G129 = -60

:

N1000 M30

Correct:

N10 G00 X0 Y0 Z0

N20 G129 = 60

:

N1000 M30

Response | Class | 1 | NC program processingContinue NC program processing. is continued.
Solution | Class | 1 | In the event of a conflict, the feed weighting is automatically set to 100%, and NC program processing is continued. Before the next program start, a meaningful value greater than zero (nil) should be programmed.
Parameter | %1: | Error value [-]
%2: | Corrected value [-]
Automatically corrected value of feed weighting
Error type | 1, Error message from NC program.