# Position preset

Select: #PSET <axis_name> <Neue Istposition> ...

This NC command can assign a new actual value to the current axis position. The resulting offset is called the position preset.

Position preset

Effectiveness

- Active until deselected or up to program end.
- Position reset is cancelled by a homing run (G74).
- A new offset has no effect until the next absolute programmed position (G90).

Deselect: #PRESET {<axis name><Dummywert>}

The position presets are cancelled in all axes if #PRESET is programmed without specifying an axis.