# ID 20118

Double programmed unit declarations.
Description | In the same NC block, more than one G function was programmed from the group of units (G70/G71). Example: Wrong: N10 G00 X0 Y0 Z0 N20 G70 X100 G71

:

N1000 M30

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify NC program. Remove the inadmissible G function.
Parameter | %1: | Error value [-]
Number of the incorrectly programmed G function
Error type | 1, Error message from NC program.