# ID 1701

Single axis is commanded but not configured in axis data list.
Description | The commissioned axis is not configured as a single axis. To use the axis as a single axis, parameter P-AXIS-00457 must be set.
Response | Class | 0 | Movement stop.
Solution | Class | 0 | Check and enable the axis parameter P-AXIS-00457
Parameter | %1: |
Logical axis number of single axis P-AXIS-00016
%2: |
Block number
%3: |
Function block ID of PLCopen Part 1
Error type | -