# ID 13111

Relative machining depth is zero (nil).
Description | The machining depth must be defined either as absolute or as relative. This message is generated when the input parameter is assigned the value zero while using a relative machining depth.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | For a relative machining depth, program the input parameter with a value unequal to zero.
Error type | 1, Error message from NC program.