# Denominator weighting factor for feedforward control (P-AXIS-00229)

P-AXIS-00229 | Denominator weighting factor for feedforward control
Description | This parameter describes the weighting factor for velocity and acceleration feedforward control.
Parameter | vorsteuer.vs_v_nenner
Data type | SGN32
Data range | 0 ≤ vs_v_nenner ≤ MAX(SGN32)
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | 1
Drive types | ----
Remarks | We know from experience that the weighting factor should be in the range of 0.7 - 1. At values >1 the axis leads and impairs contour accuracy.