# Weighting factor for speed (P-CHAN-00192)

P-CHAN-00192 | Weighting factor for speed (path-dependent dynamic weighting)
Description | This parameter defines the weighting factor for speed under index i.
Parameter | dynamic_weighting[i].velocity_fact
Data type | UNS32
Data range | 10 < velocity_fact < MAX(UNS32)
Dimension | 0.1%
Default value | 0
Remarks | Either the rapid traverse velocity and/or the maximum velocity is weighted depending on P-CHAN-00190.