# Number of axes in each axis group (P-CHAN-00003)

P-CHAN-00003 | Number of axes in each axis group
Description | This parameter defines the number of axes in an axis group. Only defined axes are counted; gaps in the axis configuration are not considered.
Parameter | gruppe[i].achs_anzahl
Data type | UNS16
Data range | 0 ... 32 (maximum number of axes, application-specific)
Dimension | ----
Default value | 0
Remarks | Only axis configurations with one axis group (gruppe[0].*) are permitted. Parameterisation example: gruppe[0].achs_anzahl 3