# Handwheel data (hr_data[i].*)

The configuration data for existing handwheels are stored in the structure 'hr_data[i]'.

Structure name | Index
hr_data[i] | i = 0 ... 5 (number of handwheels: 6, application-specific)

## Additional information

- Logical handwheel number (P-MANU-00002)
- Access to handwheel counter address (P-MANU-00003)
- Handwheel counter address (P-MANU-00004)
- Handwheel resolution
- Upper limit for handwheel increments (P-MANU-00007)
- Offset on activation (P-MANU-00012)
- Processing handwheel increments (P-MANU-00013)