# ID 120176

Pitch can not be reached due to limit in axis dynamic.
Description | With turning function thread cutting (G33), the requested pitch cannot be realized due to axes dynamic limiting. For more information on turning functions see [PROG// Section: Turning functions].
Response | Class | 1 | None.
Solution | Class | 1 | Use smaller pitch value in CNC program.
Parameter | %1: | Current value [1µm/s or 0,001°/s]
Required path velocity of face turning and longitudinal turning axis to realize requested pitch.
%2: | Limit value [1µm/s or 0.001°/s]
Maximum permissible path velocity of face turning and longitudinal turning axis.
Error type | 1, Error message from NC program.