# Associate compensation to channel (P-VOLC-00019)

P-VOLC-00019 | Associate compensation to channel
Description | This parameter specifies whether compensation is to be linked to the channel in which it was enabled. This flag impacts on the behaviour of the compensation at the end of the program, among other things. See [FCT-C26].
Parameter | associate_to_channel
Data type | BOOLEAN
Data range | 0/1
Dimension | ----
Default value | 0
Remarks |