# ID 13322

An invalid number of matrix columns has been passed to a cycle of the linalg package.
Description | When the cycle was called, an invalid number of matrix columns was transferred.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Check parameter setting and correct input parameters for the number of matrix columns.
Parameter | %1: | Identification number
Index of incorrect parameter
%2: | Upper limit value
Transferred number of columns
%3: | Current value
Required minimum number of columns
%4: | Current value
Maximum highest number of columns
Error type | 1, Error message from the NC program