# ID 120498

No workspace monitoring if CS is active.
Description | With active machine coordination system (#CS ON), no workspace monitoring can take place according to the current development status. This function will be developed in the future. For actual status ask your controller supplier.
Response | Class | 6 | Movement stop.
Solution | Class | 6 | Disabled the CS function
Error type | 1, Error message from NC program.