# Default settings at program start (prog_start.*)

The elements of this structure can initialise G, M, F and additional functions at program start. The functions are therefore grouped according to their functionality.

If no values are specified for a group in the channel parameter list, the default settings are used.

## Additional information

- Initialisation of G functions (prog_start.g_gruppe[i].*)
- Initialisation of M functions (prog_start.m_gruppe[i].*)
- Initialisation of slope parameters (prog_start.slope.*)
- Initialisation of default feed rate (P-CHAN-00099)
- Initialisation of feed rate unit (P-CHAN-00108)
- Late synchronisation at program end (P-CHAN-00033)
- Settings for Job Manager mode