# NC program paths (path[i].*)

This structure element defines the paths to the NC programs for each channel. The path string, the logical path number, the path type and priority must be specified for each program path.

## Notice

As of CNC Build V3.1.3025.05, program paths can also be defined in the channel parameters. In this case, the program paths are removed from the start-up parameters.

Further information on program paths in the channel: [CHAN//NC program paths (path[i].*)]

Structure name | Index
pfad[i] | i = 0 ... 11 (channel index, e.g. Channel 1 -> Index 0, maximum number of channels: 12, application-specific)

## Additional information

- Path specification (P-STUP-00018)
- Logical path number (P-STUP-00019)
- Path type (P-STUP-00020)
- Priority (P-STUP-00021)