# ID 120096

Selection of spline not possible in this state.
Description | Activation of spline interpolation only possible if function is inactive. For more information on spline interpolation see [PROG// Section: Akima spline interpolation].
Response | Class | 2 | Program execution stop.
Solution | Class | 6 | Check CNC program, deselect spline function via G150.
Parameter | %1: | Current value [-]
Error type | 1, Error message from NC program.