# ID 50778

Z-plane definition incorrect / minimum greater than maximum.
Description | The description of the commanded areas is incorrect. The minimum value of the Z planes is greater than the maximum value. Constant limit values for the Z-direction can be specified as limit values in the Z-plane. See also [PROG// Monitoring the work and protection area] and [FCT-C14// Description].

Example:

%zmin_zmax

N10 #CONTROL AREA BEGIN…. MIN_EXCUR=55 MAX_EXCUR=-20]

(> error

Solution:

%zmin_zmax

N10 #CONTROL AREA BEGIN…. MIN_EXCUR=-20 MAX_EXCUR=55]

(> correct

Response | Class | 6 | Movement stop.
Solution | Class | 6 | Correct the limit values for z plane
Parameter | %1: | Identification number [-]
Area ID
%2: | Lower limit value [0.1 10^-3 mm or ø]
Lower limit of the Z plane
%3: | Upper limit value [0.1 10^-3 mm or ø]
Upper limit of the Z plane
Error type | 1, Error message from NC program.