# ID 50616

The velocity of the conveyor belt is greater than the rapid feed in direction of belt.
Description | The velocity of the conveyor belt CONV_VEL specified in the #SYNC IN command exceeds the rapid traverse velocity of the axis parallel to the conveyor belt.
Response | Class | 6 | Movement stop.
Solution | Class | - |
Parameter | %1: | Logical axis number [-]
Number of the axis in the conveyor belt direction
%2: | Current value [µm/s]
Programmed conveyor belt velocity
%3: | Upper limit value [0.1 µm/s]
Maximum velocity of the belt axis in rapid traverse
Error type | -