# Struct CONTOUR_AXIS_DATA_V1

## Description

Axis-specific data of contour visualisation.

Element | Type | Meaning
act_cmd_pos | signed long int | ACS command position of the axis.
act_cmd_pos_wcs0 | signed long int | WCS_0 command position of the axis. Only calculated if the channel parameter P-CHAN-00145 has the value 1 and P-CHAN-00032 has a value > 0.
axis_nbr | unsigned short int | Axis number.
fillup | unsigned short int | Fill bytes for structure alignment