# ID 110351

Maximum velocity for axis which is not homed is greater than maximum axis velocity.
Description | The maximum velocity P-AXIS-00268 for the non-homed axis is greater than the maximum axis velocity.
Response | Class | 1 | Value is limited to maximum velocity.
Solution | Class | 1 | Correct the parameter list.
Parameter | %1: | Logical axis number [-]
P-AXIS-00016
%2: | Current value [1µm/s or 0.001°/s]
P-AXIS-00268
%3: | Limit value [1µm/s or 0.001°/s]
P-AXIS-00212
%4: | Corrected value [1µm/s or 0.001°/s]
P-AXIS-00268
Error type | 2, Error message on data transfer of parameter lists to controller.