# ID 50169

During block search not allowed interpolator control data received.
Description | When the block search function is active, some functions or functionalities, such as manual mode or homing, are not supported. For further information see FCT-C6.
Response | Class | 1 | None.
Solution | Class | 1 | Remove function selection for reported block number from the NC program.
Error type | 1, Error message from NC program.