# ID 90098

Deselection of tool radius compensation while contour masking process is active.
Description | TRC is deselected without first deactivating contour masking.
Response | Class | 1 | NC program processing is continued
Solution | Class | 1 | Modify the NC program: Deselect contour masking before deselecting the TRC
Parameter | %1: | Block number [-]
Block number of TRC deselection.
Error type | 1, Error message from NC program.