# ID 20822

Parameters must be programmed for the definition of an (A)CS.
Description | When defining a machining coordinate systems (#CS DEF) or a coordinate system for fixture adaptation (#ACS DEF), it is essential to program the parameters for translation and rotation. [PROG// Section: Defining a machining coordinate system (CS)]

[PROG// Section: Defining/activating a coordinate system for fixture adaptation (ACS)]

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check the command #(A)CS DEF, complete the parameters for translation rotation.
Error type | 1, Error message from NC program.