# ID 110288

Changing the hardware counter id requires a restart.
Description | The parameter P-AXIS-00042, that indicates the unique hardware identification of the counter numerator, cannot be changed while CNC kernel is running. The new hardware identification is not transferred, the previous active hardware identification remains valid.
Response | Class | 1 | None.
Solution | Class | 1 | Change the entry P-AXIS-00042 only in configuration mode or when CNC is disabled.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Current value [-]
Current value of P-AXIS-00042.
%3: | Corrected value [-]
Corrected value of P-AXIS-00042.
Error type | 2, Error message by data transfer from parameter list into control device.