# ID 20889

Channel parameters: Face-ID is out of range of permissible values.
Description | During start-up, the entry for the facing ID is checked for its valid value range. The value of the Face ID P-CHAN-00008 in the channel parameters list is out of range.
Response | Class | 1 | Controller start-up is continued.
Solution | Class | 1 | Check and modify the value of the Face ID P-CHAN-00008 in the channel parameters before the next controller start-up. In case of conflict, the value of Face D is set to the maximum limit at start-up.
Parameter | %1: | Error value [-]
Invalid value of Face ID in channel parameter list
%2: | Upper limit value [-]
Maximal value of Face ID
%3: | Corrected value [-]
Value of Face ID automatically corrected
Error type | 2, Error message by data transfer from parameter list into control device.