# ID 20434

Channel parameters: The characteristic of P-parameters is not configured.
Description | During start-up, the channel parameter check determines that the effectiveness of P parameters P-CHAN-00067 is not defined.
Response | Class | 1 | Start-up of the control is continued.
Solution | Class | 1 | In the event of a conflict, the effectiveness of P parameters P-CHAN-00067 is set to 0 (FALSE) during the start-up and the start-up is continued. P-CHAN-00067 must be assigned 0 (FALSE) or 1 (TRUE).
Parameter | %1: | Error value [-]
%2: | Corrected value [-]
Error type | 2, Error message by data transfer from parameter list into control device.