# Programmed M00 stop during backward movements (P-CHAN-00276)

P-CHAN-00276 | Programmed M00 stop during backward movements
Description | Suppress stop during backward movements with M00.
Parameter | forward_backward.disable_m00_backward
Data type | BOOLEAN
Data range | 0: The process also stops in the backward direction with M00. 1: Stopping with M00 is omitted in the backward direction.
Dimension | ----
Default value | 0
Remarks |