# ID 20475

Master axis can not be its own slave axis.
Description | With the definition of a coupling group it is detected, that one of the master axis also is its own slave axis. Example: Wrong: N10 G00 X0 Y0 Z0 N20 #SET AX LINK[1,X=X]

:

N1000 M30

For further information see [PROG// Section: Programming axis couplings]

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify NC program. Master axis and slave axis must not be identical. Observe the restrictions regarding master/slave axes dependence[PROG//Section: Synchronous mode].
Parameter | %1: | Logical axis number [-]
Axis number of the invalid axis
%2: | Current value [-]
Index of the coupling pair
%3: | Current value [-]
Number of the coupling group
Error type | 1, Error message from NC program.