# ID 21908

Incomplete contour path can not be given out.
Description | Contour path of 2 blocks is programmed. Too many control and/or technology blocks were programmed between the two blocks of the contour section that the controller is forced to output blocks. Since the contour section is only complete when the second block is presented, it can neither be determined nor output.

Solution proposed:

Reduce number of blocks between the relevant blocks of contour path.

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the NC program.
Error type | 1, Error message from NC program.