# ID 20803

Temporary transition into machine coordinate system is already enabled.
Description | Multiple selection of the temporary transition to the machine coordinate system with the command #MCS ON has no effect since the temporary transition is already enabled.
Response | Class | 1 | Continue NC program processing.
Solution | Class | 1 | Remove the repeated programming of the #MCS ONcommand.
Error type | 1, Error message from NC program.