# ID 60164

Error in table manager function
Description | An error occurred while using camming tables.
Response | Class | 5 | Abort command/NC-Program.
Solution | Class | 6 | Read parameter No.3 and contact service personal.
Parameter | %1: |
Logical axis number (P-AXIS-00016) of the spindle
%2: | Identification number [-]
ID of CAM table that you want to access.
%3: | Current value [-]
Error identifier.
Error type | -