# ID 20418

Channel parameters: Number of spindles and number of configured spindle axes do not match.
Description | During start-up, the channel parameter check determines that the actual number of configured spindles (spindle data) does not correspond to the total number of spindles P-CHAN-00082.
Response | Class | 1 | Start-up of the control is continued.
Solution | Class | 1 | During start-up in case of conflict the total number of spindles is set to the real number of configured spindles and the start-up is continued.
Parameter | %1: | Current value [-]
Total number of spindles P-CHAN-00082
%2: | Expected value [-]
Real number of configured spindles (spindle data)
%3: | Corrected value [-]
Automatically corrected total number of spindles
Error type | 2, Error message by data transfer from parameter list into control device.