# Programmed M01 stop during backward movement (P-CHAN-00278)

P-CHAN-00278 | Programmed M01 stop during backward movement
Description | Suppress stop during backward movement with M01.
Parameter | forward_backward.disable_m01_backward
Data type | BOOLEAN
Data range | 0: The process also stops in backward direction with M01. 1: Stopping with M01 is omitted in the backward direction.
Dimension | ----
Default value | 0
Remarks |