# ID 50870

Shift of control block not done.
Description | In connection with the #SHIFT functionality, the interpolator must hold back motion blocks until the shift operation is completed. In the present case, it was detected that the required shift operation was not executed when one of the technology functions to be shifted was crossed.
Response | Class | 4 | Movement stop.
Solution | Class | 6 | Please contact the control manufacturer.
Error type | 1, Error message from NC program.